**DNF Controllers**

**Routing to PLAY DNF Controller**

* In X-Y Mode only, route to desired QC station. Ex QC\_2. (Note deck must be in remote)

**Routing to RECORD DNF Controller**

* In X-Y Mode only, route to desired QC station with an A at the end. Ex QC\_2A. (Note deck must be in remote)

**Gang Control**

* From MultiDest, press the [HOLD PST] button to make multiple selections at once.
* Using the buttons below the LCD screen, use [PAGE UP] and [PADE DN] to navigate through the racks to select all of your record decks.
* Once all of your decks are selected, hit the [BROADCAST] button.
* Next route your desired RECORD DNF Controller. Ex QC\_2A and press [TAKE]. (Note: you won’t see the QC appear in the preset column.)
* As long as the 9 pin remote is turned on all of your record decks, you should now be able to control them all at once from the RECORD DNF Controller at your station.