DVCPRO HD Deck Settings

**Configuring Deck for NTSC or PAL Reference**

1. Press the “[Menu]” button on the deck’s panel.
2. Press the “[F]” button and “System [F4]” button at the same time.
3. Change **25 SYSTEM FREQ** settings using the “[adjust]” knob on the front panel. Press the knob in to enter and save selection.
	1. 59/60 for NTSC (59.94)
	2. 50i/25p for PAL (50)
4. Press “Set [F5]” to save changes.
5. The reference must match the deck setting. Ex: If the setting is PAL, you must have PAL routed into the deck.

**Configuring the Deck’s Resolution**

1. Press the “[Menu]” button on the deck’s panel.
2. Press the “[F]” button and “Setup [F5]” button at the same time.
3. Change **020 SYS FORMAT** to 720p or 1080i using the “[adjust]” knob on the front panel. Press the knob in to enter and save selection
4. Press “Set [F5]” to save changes.
5. The resolution must match the deck setting. Ex: If the setting is 1080i, you must have 1080i routed into the deck.

**Configuring the Deck’s Internal Cross Converter**

1. Press the “[Menu]” button on the deck’s panel.
2. Press the “[F]” button and “Setup [F5]” button at the same time.
3. Change the following settings based on your tape masters resolution and desired output. Use the “[adjust]” knob on the front panel to change settings. Press the knob in to enter and save selection
	1. **630 1080i > HD\_OUT**
		1. Select 1080i to have no conversion
		2. Select 720p to cross convert from 1080i>720p
	2. **632 720p > HD\_OUT**
		1. Select 720p to have no conversion
		2. Select 1080i to cross convert from 720p>1080i
4. Press “Set [F5]” to save changes.