HD Decks Marked w/ Red Tape

* VTR 1233 (D5)
* VTR 1234 (D5)
* VTR 1243 (DVCPRO)
* VTR 1244 (DVCPRO)
* VTR 1253 (DVCPRO)
* VTR 1254 (DVCPRO)

These decks have the following extra functionality:

* Built in Down Converters
* Ability to output Burned in Timecode (BITC)

Note: To access the SD outputs of these decks and use the below settings, you must route with an “S” at the end of the VTR number. Ex: VTR 1233 would be VTR 1233s.

**D5 Down Converter Settings**

1. Press the Video “Out” on button on the deck’s panel
2. Select “Convert [F10]”
3. Select “HD to SD [F1]”
4. Select “Mode [F1]” to change your down convert options
   * FIT H = 16x9 Letterbox
   * FIT V = 4x3 Center Cut
   * FIT H&V = 16x9 Anamorphic

**D5 BITC Settings**

1. Press the “TC/CHR” button on the deck’s panel.
2. Select “Super [F11]” to toggle on or off. Use “TC” setting for BITC (Note: Make sure your TC/CTL button (F4) on the Home screen is set to TC, NOT CTL)

**DVCPRO HD Down Converter Settings**

1. Press the “Video” button on the deck’s panel.
2. Select “Dw Con [F6]” to change your down convert options
   1. FIT H = 16x9 Letterbox
   2. FIT V = 4x3 Center Cut
   3. FIT H&V = 16xp Anamorphic
3. (Note: Make sure your TC/CTL button (F3) on the Home screen is set to TC, NOT CTL)

**DVCPRO HD BITC Settings**

1. Press the “TC” button on the deck’s panel.
2. Press the “Shift” button on the deck’s panel to go to the next row of TC settings.
3. Select “Super [F1]” to toggle BITC on or off.
4. “DISPLY [F4]” should be set to “Time” for BITC.